**ITEM NO: VT-1212; WATTS: 12W**



|  |  |
| --- | --- |
| Item No: | VT-1212 |
| SKU Codes | **4268:6000K** |
| Type | **PAR30** |
| Base | **E27** |
| Real Watts | **12W** |
| EQ. Watts | **60W** |
| Voltage | **220~240V** |
| Input Frequency | **50Hz** |
| Input Efficiency | **62lm/w** |
| Lumen(lm) | **750lm** |
| PF | **>0.5** |
| CRI | **>80** |
| Color Temperature | **3000K,4500K,6000K** |
| Beam Angle | **40’D** |
| LED Chip | **SMD** |
| Driver | **Constant Current Non-Isolated Driver** |
| Protection Class | **IP20** |
| Body Material | **Plastic** |
| Dimmable | **No** |
| Unit size | **95mmx114mm** |
| Life Time | **20000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |