**LED STRIPS**

**Item no:VT-3528/60**



|  |  |
| --- | --- |
| Item No: | VT-3528/60 |
| Real Watts | **24W/5M** |
| Voltage | **DC 12V** |
| Input Frequency | **50/60Hz** |
| Input Current | **2A/5M** |
| Lumen/LED | **4:5** |
| Color Temperature | **White, Warm White, Red, Green, Blue** |
| Beam Angle | **120’D** |
| LED Chip | **SMD 3528** |
| LED Qty | **300/5M** |
| Driver | **No** |
| Protection Class | **IP20/IP65** |
| Unit size | **5 Mtr; Width:8mm** |
| Life Time | **20000hrs** |
| Outside using temperature | **-20 ~50’C** |
| Packing Method | **5mtr roll/packing** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |